|  |  |
| --- | --- |
| **leave-one-X-out**  **setup** | **average RFr**  **accuracy** |
| layer | 0.93 |
| spacing | 0.96 |
| speed | 0.75 |
| pressure | 0.36 |
| speed-pressure | 0.75 |

**TableX.** RFr models were evaluated and the  
average accuracy is reported. Models were  
trained in different leave-one-out settings.  
The test set was developed to contain one  
layer, spacing, speed, pressure value and   
speed-pressure value combination.